PALETTEENTRY

类型定义
Type PALETTEENTRY ' 4 Bytes peRed As Byte peGreen As Byte peBlue As Byte peFlags As Byte End Type
说明
Describes an entry in a logical palette
字段表
字段 | 类型与说明
peRed | Byte，An 8-bit value describing the red component of an RGB color.
peGreen | Byte，An 8-bit value describing the green component of an RGB color.
peBlue | Byte，An 8-bit value describing the blue component of an RGB color.
peFlags | Byte，An 8-bit value containing one of the following values: 0: Map this entry normally. PC_EXPLICIT: The low order word (combination of the peRed and peGreen fields) contains an index into the system palette. This allows you to display the system palette colors. PC_NOCOLLAPSE: This color is mapped into an unused system palette entry and will not be mapped to an existing color. Subsequent palettes may map colors to this entry. PC_RESERVED: This color is mapped to an unused system palette entry and no other logical palettes will be mapped to that entry. By restricting the system palette entry to this logical entry, color cycling involving direct changes to the system palette becomes possible.

Top