By default RivaTuner follows AGP 3.0 specifications and never uses display adapter's and northbridge's SBA_ENABLE bits to detect actual state of SBA.
However, you may force RivaTuner to use AGP2.0-styled SBA detection by settings this entry to 1.