Use this value to force RivaTuner to initiate task switching after each I2C transaction. Task switching may prevent other applications not supporting I2C access synchronization protocol from loosing their I2C transactions and misreading data.