This value allows you to force RivaTuner to exclude Horizontal / Vertical span modes from the list of supported display modes when applying 60Hz fix.
By default RivaTuner excludes span modes on single head display adapters in order to work around the Detonator's NV_Modes decompression bug.