This bitmask allows unlocking both read (bit 0) and write (bit 1) access modes for the automatic fan speed adjustment rule on LM63 and ADT7473 compatible fan controllers. Set this value to 3 to get full access to automatic fan speed adjustment rule parameters.



