RivaTuner checks this value when restoring clock frequencies after resuming from suspended mode under Windows2000/XP. The clock frequenices will be restored immediately after logging in when this value is set to 1, otherwise they will be restored after the first display mode switch.
