This value controls fake DDR heuristic detection algorithm. Set this value to 1 to forcibly activate it and treat MPLL frequency as incorrectly doubled. Set it to 0 to forcibly disable it and always display the real MPLL frequency.