Some fan controllers (e.g. ADT7473) need some time to reflect actual duty cycle change after switching from automatic to fixed fan control mode and vice versa. 
That is why RivaTuner perform fan controller type specific delay between applying new fan settings and refreshing GUI. You may use this value to redefine this delay (in 500ms units).