Some settings (e.g. overclocking and fan control) cannot be applied independently to the primary and secondry heads of dual-head display adapters and are available for the master head display device only. By default RivaTuner maps GUI of the secondary display devices to the master display device for such settings. You may use this value to override such behavior.