This plugin provides [cff][b]Core temperature[/b][/c], [cff][b]Ambient temperature[/b][/c], [cff][b]Fan duty cycle[/b][/c], [cff][b]Fan speed[/b][/c] and voltage hardware monitoring data sources for display adapters with Fintek F75373S-compatible sensors. The voltages are displayed as [cff][b]Vcc[/b][/c] and raw [cff][b]V1[/b][/c] - [cff][b]V3[/b][/c] sensor's inputs readings if display adapter doesn't exist in plugin's voltage calibration database, otherwise plugin automatically maps raw voltage inputs to [b][cff]Vcc[/b][/c], [b][cff]AGP Vddq[/b][/c], [b][cff]Vcore[/b][/c] and [b][cff]FB Vddq[/b][/c] and transparently performs required voltage reading correction.

[b]Tips:[/b]
-F75373S-compatible sensors are used on ASUS V9999 and X800 series.
-Due to VGA BIOS design flaws some F75375S capable ASUS display adapters are unable to report core temeprature properly when generic ASUS SmartDoctor software is not installed. To avoid this problem, the plugin provides optional [b][cff]BJT calibration[/b][/c] mode, performing the same sensor calibration like SmartDoctor software. To enable the calibration you may set [cff][b]CalibrateTemperatureBJT0[/b][/c] to 1 in [cff][b]Settings[/b][/c] section of F75373.cfg file.
