Home ·

# SAM9X60Config QML Type

Contains configuration values for a SAM9X60 device. More...

Import Statement: | import SAMBA.Device.SAM9X60 3.7

- List of all members, including inherited members

## Properties

- extram : alias
- lowlevel : alias
- nandflash : alias
- qspiflash : alias
- sdmmc : alias
- serial : alias
- serialflash : alias
- setgpio : alias

## Detailed Description

By default, no configuration values are set.

## Serial Console Configuration

The following serial console configurations are supported:

Instance | Peripheral | I/O Set | TX Pin
--- | --- | --- | ---
0 | DBGU | 1 | PA10A
1 | FLEXCOM0 | 1 | PA0A
2 | FLEXCOM1 | 1 | PA5A
3 | FLEXCOM2 | 1 | PA7A
4 | FLEXCOM3 | 1 | PC22B
5 | FLEXCOM4 | 1 | PA12A
6 | FLEXCOM5 | 1 | PA22B
7 | FLEXCOM6 | 1 | PA30A
8 | FLEXCOM7 | 1 | PC0C
9 | FLEXCOM8 | 1 | PB4B
10 | FLEXCOM9 | 1 | PC8C
11 | FLEXCOM10 | 1 | PC16C
12 | FLEXCOM11 | 1 | PB19C
13 | FLEXCOM12 | 1 | PB21C

## External RAM

The following external RAM configurations are supported:

Preset | Type | Model | Size
--- | --- | --- | ---

## SD/MMC Configuration

The following SD/MMC configurations are supported:

Instance | Peripheral | I/O Set | Bus Width
--- | --- | --- | ---
0 | SDMMC0 | 1 | 1-bit, 4-bit
1 | SDMMC1 | 1 | 1-bit, 4-bit

The SD/MMC applet on SAM9X60 does not support voltage switching, so the voltage configuration property is ignored.

### Pin List for SD/MMC Instance 0 (I/O Set 1)

Pin | Use
--- | ---
PA17A | Clock
PA16A | Command
PA15A | Data 0 (bus width: 1-bit, 4-bit)
PA18A | Data 1 (bus width: 4-bit)
PA19A | Data 2 (bus width: 4-bit)
PA20A | Data 4 (bus width: 4-bit)

### Pin List for SD/MMC Instance 1 (I/O Set 1)

Pin | Use
--- | ---
PA13B | Clock
PA12B | Command
PA11B | Data 0 (bus width: 1-bit, 4-bit)
PA2B | Data 1 (bus width: 4-bit)
PA3B | Data 2 (bus width: 4-bit)
PA4B | Data 3 (bus width: 4-bit)

## SPI Serial Flash Configuration

The following SPI Serial Flash configurations are supported:

Instance | Peripheral | I/O Set | Chip Selects
--- | --- | --- | ---
0 | FLEXCOM0 | 1 | 0, 1
1 | FLEXCOM1 | 1 | 0, 1
2 | FLEXCOM2 | 1 | 0, 1
3 | FLEXCOM3 | 1 | 0, 1
4 | FLEXCOM4 | 1 | 0, 1, 2, 3
4 | FLEXCOM4 | 2 | 0, 1, 2, 3
5 | FLEXCOM5 | 1 | 0, 1, 2, 3
5 | FLEXCOM5 | 2 | 0, 1, 2, 3

### Pin List for SPI Serial Flash Instance 0 (I/O Set 1)

Pin | Use
--- | ---
PA0A | MOSI
PA1A | MISO
PA4A | SPCK
PA3A | NPCS0
PA2A | NPCS1

### Pin List for SPI Serial Flash Instance 1 (I/O Set 1)

Pin | Use
--- | ---
PA5A | MOSI
PA6A | MISO
PC29C | SPCK
PC28C | NPCS0
PC27C | NPCS1

### Pin List for SPI Serial Flash Instance 2 (I/O Set 1)

Pin | Use
--- | ---
PA7A | MOSI
PA8A | MISO
PB2B | SPCK
PB1B | NPCS0
PB0B | NPCS1

### Pin List for SPI Serial Flash Instance 3 (I/O Set 1)

Pin | Use
--- | ---
PC22B | MOSI
PC23B | MISO
PC26B | SPCK
PC25B | NPCS0
PC24B | NPCS1

### Pin List for SPI Serial Flash Instance 4 (I/O Set 1)

Pin | Use
--- | ---
PA12A | MOSI
PA11A | MISO
PA13A | SPCK
PA14A | NPCS0
PA0C | NPCS1
PA1B | NPCS2
PB3B | NPCS3

### Pin List for SPI Serial Flash Instance 4 (I/O Set 2)

Pin | Use
--- | ---
PA12A | MOSI
PA11A | MISO
PA13A | SPCK
PA14A | NPCS0
PA7B | NPCS1
PA8C | NPCS2
PB3B | NPCS3

### Pin List for SPI Serial Flash Instance 5 (I/O Set 1)

Pin | Use
--- | ---
PA22B | MOSI
PA21B | MISO
PA23B | SPCK
PA8B | NPCS0
PA0B | NPCS1
PA31B | NPCS2
PA30B | NPCS3

### Pin List for SPI Serial Flash Instance 5 (I/O Set 2)

Pin | Use
--- | ---
PA22B | MOSI
PA21B | MISO
PA23B | SPCK
PA8B | NPCS0
PA7C | NPCS1
PA31B | NPCS2
PA30B | NPCS3

## QSPI Flash Configuration

The following QSPI Flash configurations are supported:

Instance | Peripheral | I/O Set
--- | --- | ---
0 | QSPI0 | 1

### Pin List for QSPI Serial Flash Instance 0 (I/O Set 1)

Pin | Use
--- | ---
PB19A | SCK
PB20A | CS
PB21A | IO0
PB22A | IO1
PB23A | IO2
PB24A | IO3

## NAND Flash Configuration

The following NAND Flash configurations are supported:

I/O Set | Bus Width
--- | ---
1 | 8-bit, 16-bit

### Pin List for NAND Flash (I/O Set 1)

Pin | Use | Bus Width
--- | --- | ---
PD0A | NANDOE | 8-bit, 16-bit
PD1A | NANDWE | 8-bit, 16-bit
PD2A | NANDALE | 8-bit, 16-bit
PD3A | NANDCLE | 8-bit, 16-bit
PD4A | NCS3 | 8-bit, 16-bit
PD5A | NWAIT | 8-bit, 16-bit
PD6A | D16 | 8-bit, 16-bit
PD7A | D17 | 8-bit, 16-bit
PD8A | D18 | 8-bit, 16-bit
PD9A | D19 | 8-bit, 16-bit
PD10A | D20 | 8-bit, 16-bit
PD11A | D21 | 8-bit, 16-bit
PD12A | D22 | 8-bit, 16-bit
PD13A | D23 | 8-bit, 16-bit
PD14A | D24 | 16-bit
PD15A | D25 | 16-bit
PD16A | D26 | 16-bit
PD17A | D27 | 16-bit
PD18A | D28 | 16-bit
PD19A | D29 | 16-bit
PD20A | D30 | 16-bit
PD21A | D31 | 16-bit

## Property Documentation

extram : alias

Configuration for external RAM applet

See ExtRamConfig for a list of configurable properties.

lowlevel : alias

Configuraiton for Low Level applet

see LowlevelPresetConfig for a list if configurable properties.

nandflash : alias

Configuration for NAND Flash applet

See NANDFlashConfig for a list of configurable properties.

qspiflash : alias

Configuration for QSPI Flash applet

See QSPIFlashConfig for a list of configurable properties.

sdmmc : alias

Configuration for SD/MMC applet

See SDMMCConfig for a list of configurable properties.

serial : alias

Configuration for applet serial console output

See SerialConfig for a list of configurable properties.

serialflash : alias

Configuration for SPI Serial Flash applet

See SerialFlashConfig for a list of configurable properties.

setgpio : alias

Configuration for Set GPIO applet