0x01,Pretest Fail,It's good MU not equal to total MU
0x02,Check Size Fail,It's flash size not equal to specific value.
0x03,Write CID Fail,CID pattern verify fail
0x04,Download ISP Fail,ISP pattern verify fail
0x05,Copy Compare Fail,There are some data not match.
0x06,Format Fail,MBR/PBR pattern verify fail.
0x07,Make AutoRun Fail,ISO file write fail
0x08,Device Write Protect,Device can't access.
0x09,Preload Fail,There is a compare or file not found error when copy file into UFD.
0x0A,Write CID2 Fail,CID2 pattern verify fail
0x0B,Update WPRO fail,Mutli-lun partition fail
0x0C,Reset Fail,Software reset CPU fail
0x0D,Check Info Block Fail,Check Info Block Fail (Before Download ISP)
0x0E,SM3257ENBA Download ISP Fail,
0x0F,Initial Fail,Initial parameter and reference data fail
0x10,Error Bits Over Fail,Error Bits Are Too Much Over Threshold
0x11,Bad block over Setting,Total bad block over the BBOption.
0x12,Check Open/Short Fail,Check Open/Short Fail
0x13,Pre-scan Early Bad Fail,Pre-scan Early Bad Fail
0x14,Specific Bad Block Fail,Specific Bad Block Fail
0x15,Check Data Shaping Fail,Check Data Shaping Fail
0x16,Check USB Mode Fail,USB1.1/2.0 checking fail.
0x17,Update SN After pass Fail,The serial write fail
0x18,Check Spare Count Fail,Count of spare block is less
0x19,Extern Serial Number EOF Fail,Serial Number in extern file is no more for using
0x1A,Device Removed before pass/fail,Device off-line
0x1B,Device new bad,Device add new bad fail
0x1C,Flash Can Not Support DDR,Force DDR option usage 
0x1D,DDRTest.BIN Can Not Find,Force DDR option usage 
0x1E,ConvertFlashID.BIN Can Not Find,Convert Flash ID option usage 
0x1F,Convert FlashID Fail,Convert Flash ID option usage 
0x20,Check Windows To Go Size Fail ,Check Windows To Go Size Fail 
0x21,Check Windows To Go Format Fail ,Check Windows To Go Format Fail 
0x22,Chip Not Support Windows To Go (Accept SM326X Series),Check Windows To Go device
0x23,Check Spare Block Fail (Size Is Zero),Check space block status
0x24,Check Windows To Go Spare Size Fail,Check Windows To Go space block status.
0x25,Check Serial Number Length Fail,Check serial number length when user enables this option.
0x26,Cannot Find DLL When Enable Decode BCH Flag,Specific DLL file not found 
0x27,Cannot Find Block When Decode BCH,Enable decode bad block option, but can't find any information data. 
0x28,Detects HDD device, It Cannot Support NTFS Format,HDD device without letter, it cannot support NTFS format.
0x29,Prescan.BIN Can Not Find,Pre-scan bad blocks option usage
0x2A,Pre-scan Bad Blocks Fail,Pre-scan bad blocks option usage
0x2B,Change USB Speed Fail,326x change USB speed (U2 -> U3 or U3 -> U2) fail
0x2C,BadBitTable.bin or BadByteTable.bin or ErrPage.bin Can Not Find,Remapping verify test usage
0x2D,Remapping Flow Fail,Remapping verify test usage
0x2E,Device Over Current,Device over current is happened.
0x2F,Device Not Find,Device is not found.
0x30,Timeout,Time out is happened.
0x31,Check flash ID doesn't match.,Check Flash ID is matched or not(4bytes)
0x32,User stop MP,User press stop procedure.
0x33,Erase Info Fail,Erase system info fail
0x35,ECC U-Correctable Fail,ECC U-Correctable Fail
0x36,Lock Content File Fail,Can't lock content files 
0x37,No Response From Device, Please Re-plug Device,Device can't find anymore.
0x38,Erase Good Error, Please Change to Erase All,Please select correction erase mode.
0x39,FAT32 Format Alignment Fail,Format Alignment Fail
0x3A,Read Hynix Read Retry OTP Data Fail,Read Hynix Read Retry OTP Data Fail
0x3B,Check Card Mode Fail,Check Card Mode Fail
0x3C,Check All CEs Are Not Same Fail,Check All CEs Are Not Same Fail
0x3D,Check Channel CE No Fail,Check Channel CE No Fail
0x3E,RAM Test Fail,RAM Test Fail
0x3F,Check CE Care Mode Fail,Check CE Care Mode Fail
0x40,CheckEraseStatus.bin Can Not Find,Check block 0 & 1 erase status usage
0x41,Check Erase Status Fail,Check block 0 & 1 erase status usage
0x42,Hardware SEL_C Value Fail,Check hardware SEL_C value
0x43,Flash Error Bit Is Too High,Check L84C/L95B
0x44,HW Fine Tune Fail,SM3267 hardware fine tune usage
0x45,HWFineTune.bin Can Not Find,SM3267 hardware fine tune usage
0x46,Check Controller Fail,Check Controller for Transcend Mode
0x47,Copy SN to File Fail,Write SN to a file and copy to the device fail
0x48,GenInfoCmd BIN File Can Not Find,PC Base flow usage
0x49,Load GenInfoCmd Bin File Fail,PC Base flow usage
0x4A,ChkSLCFly.bin Can Not Find,Check SLC On the Fly usage
0x4B,Check SLC On The Fly Fail,Check SLC On the Fly usage
0x4C,Die Scan Fail,Die Scan flow usage
0x4D,Occupied Fail,Check file system usage
0x4E,Download SPI Fail,SM3269AA lightning interface usage
0x4F,Check Duplicate ISP Fail,Check duplicated ISP for SM3257ENx
0x50,Check SMI Cert Fail,SMI Certification flow usage
0x51,Check Coprocessor Test Fail,SM3269 Coprocessor Test Fail
0x52,Check H2 Test File Fail,Check if there is H2 file or not
0x53,Check E-Fuse Value Fail,Check SM328x E-Fuse value
0x54,H2 Test Fail,SMI H2 Test usage
0x81,QC SCSISTR FAIL,Check SCSI Vendor Error
0x82,QC PRONAME FAIL,Check SCSI Product Error
0x83,QC CAPACITY FAIL,Check Disk Capacity Error
0x84,QC ISPSTR FAIL,Check ISP Version Error
0x85,QC VENDORSTR FAIL,Check Vendor String Error
0x86,QC PRODUCTSTR FAIL,Check Product String Error
0x87,QC VIDSTR FAIL,Check VID Error
0x88,QC PIDSTR FAIL,Check PID Error
0x89,QC USBMODE FAIL,Check USB Mode Error
0x8A,QC USBPOWER FAIL,Check USB Power Error
0x8B,QC TESTERSTR FAIL,Check Tester Version Error
0x8C,QC DBFMETHOD FAIL,Check DBF Method Error
0x8D,QC Check Disk Type FAIL,Check Disk Type Error
0x8E,QC ISP FAIL,Check ISP Error
0x8F,QC Check Disk Label FAIL,Check Disk Label Error
0x90,QC Check Disk Format FAIL,Check Disk Format Error
0x91,QC Compare CID Fail,Check CID buffer Error
0x92,QC Check Flash ID Fail,Check Flash ID buffer Error
0x93,QC Check ISP Version Fail,Check version of ISP Error
0x94,QC Compare CDROM Fail,Compare data of CDROM Error
0x96,QC CID Setting Fail,Link block number is too large
0x97,QC Check Used Space Fail,Check used space of formatted device error.
0x98,QC Check Preload Fail (Non-FAT mode),Check Preload Non-FAT Image Error
0x99,QC Check Preload Fail  (FAT mode),Check Preload FAT Files Error
0x9A,QC Check Flash ID Fail,Check Flash ID Error
0x9B,QC Compare SN Header Fail,Check Serial Number Header Error
0x9C,QC Compare SN Length Fail,Check Serial Number Length Error
0x9E,QC Check Bad Block Fail,Check Bad Block Error
0x9F,QC Check Sensor Self-Test Fail,Check Sensor Self-Test Error
0xA0,QC Check SDR/DDR Fail,Check SDR/DDR Error
0xFF,No Device,