MIDI configuration

This panel is used to configure the MIDI interfaces.

Setting | Description
Input device | Selects a MIDI input device to control the pattern editor.
Output device | Output commands to a MIDI device.
Receive sync ticks | Enable receiving MIDI timing clock, which causes the tracker to step down in the pattern editor for each 6'th tick. This results in 4 steps/quarter note.1
Skip key releases | Skip recording of key release commands.
Map MIDI to NES channels | Maps the MIDI channels to the tracker channels (MIDI channel 0 = pulse 1, channel 1 = pulse 2...)
Record velocities | Translate MIDI note velocities to volume column values.
Auto arpeggiate chords | Arpeggiate multiple keypresses.

1. Note: This command will also disable automatic step down when inserting notes in the pattern editor!

Back to configuration · interface · main index