RivaTuner does not change NVPLL post divider by default. You can allow RivaTuner to change NVPLL post divider by setting this value to 0.
It will improve clock frequency generation accuracy, but may result in reduced stability.