RivaTuner does not change MPLL post divider by default. You can allow RivaTuner to change MPLL post divider by setting this value to 0.
It will improve clock frequency generation accuracy, but may result in reduced stability.