By default RivaTuner parses VGA BIOS clock initialization scripts to change clock frequencies on ATI RADEON X1000 display adapters. You may set this entry to 0 to prevent RivaTuner from parsing VGA BIOS scripts and force it to use hardcoded GPU family specific clock frequency programming codepaths.