This value can be used to force RivaTuner to flush bitmaps used to render hardware monitoring graphs within specified period after each display mode change.
Bitmaps flushing can help display driver to optimize graphs rendering after starting and closing 3D applications. Bitmaps flushing can be disabled by setting this value to 0.