RivaTuner doesn't change MPLL reference divider by default when it's set to 1 on DDR boards. You can allow RivaTuner to change MPLL reference divider regardless of its' current state by setting this value to 0.
It will improve clock frequency generation accuracy, but may result in reduced stability.